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	TASK
	Combine harvester

	HAZARDS
	Flying debris
	☐	Heat / cold
	☐	Electricity
	☐
	
	Cuts / laceration
	☐	Exposure
	☐	Rollover
	☒
	
	Pinch / crush 
	☐	Noise / vibration
	☐	Plant interaction
	☐
	
	High pressure
	☐	Falling
	☒	Entrapment
	☒
	PPE REQUIRED
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	PRE-START CHECKS

	1. Complete pre-start check as per manufacturer’s guidelines. 
2. Ensure all safety guards and shields are in place and functioning properly.
3. Verify that all controls and systems are operational by performing a test run in a safe area.

	

	SAFE OPERATING PROCEDURE

	1. Ensure personnel are competent and authorized.
2. Ensure personnel are fit for duty and not impaired by drugs or alcohol.
3. Do not use a mobile phone while operating and always wear your seatbelt.
4. Operate at a safe speed and maintain exclusion zones around people, powerlines, and other hazards (use spotters if necessary).
5. Beware of uneven or sloping ground.
6. Use caution when turning, reversing, or operating on slopes to prevent rollovers or accidents.

	

	POST-OPERATION PROCEDURE

	1. Park the combine harvester in a designated area and turn off the engine.
2. Perform a final visual inspection for any damage or debris.
3. Clean the combine harvester and remove any residue or debris to prevent corrosion and damage.
4. Secure the combine harvester and store any detachable parts or accessories properly.
5. Report any issues or incidents encountered during operation to the appropriate personnel.
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